How are the faber-castell pencils made?

First, raw materials, clay and graphite, are mixed together.

Water is now added.

//Primero el sustantivo y después el verbo siempre en afirmaciones.

After this, pressure is applied to make/produce the pencil leads.

Now, they are dried.

A wax bath is applied.

The leads are bathed in wax.

The colour pencil leads/leads of colour pencils are made through the same process.

Now, pencils are made/ Now, it is time to make pencils.

holes are milled.

Then, glue is applied.

Now, leads are inserted.

Now each pencil is separated.

Finally, pencils are painted and stamped.

Now, paint is mixed.

Now, pencils are carried through a conveyor belt.

Pencils are dipped (sumergir).

Pencils are dried in the drying room.

Pencil strength is tested to check if they withstand over 2.5 kg of pressure.

Then, the pencils are sharpened.

Pencil sharpener -> sacapuntas.

Finally, pencils are packed/packaged.